Configuration group  
Celje WiFi

Mestna občina Celje  
  
Konfiguracija 2024-02-23

RF Group: Celje WiFi

|  |  |
| --- | --- |
|  |  |
| allowed\_channels: | 36,40,44,48,52,56,60,64,100,104,108,112,116,120,124,128,132,136,140,149,153,157,161,165 |
| beacon\_interval: | 100 |
| ch\_bw\_range: | ['20MHz', '40MHz'] |
| channel\_quality\_aware: | True |
| channel\_quality\_threshold: | 70 |
| channel\_quality\_wait\_time: | 120 |
| csa\_count: | 0 |
| disable\_arm\_wids\_functions: | off |
| dot11h: | False |
| dpp\_configurator\_connectivity: | False |
| frame\_bursting\_mode: | dynamic |
| high\_noise\_backoff\_time: | 720 |
| interference\_immunity: | 2 |
| legacy\_mode: | False |
| max\_tx\_power: | 51 |
| max\_tx\_power\_ai: | false |
| min\_tx\_power: | 38 |
| min\_tx\_power\_ai: | false |
| name: | Outdoor |
| radar\_backoff\_time: | 720 |
| rts\_mode: | default |
| scanning\_disable: | True |
| smart\_antenna: | False |
| spectrum\_band: |  |
| spectrum\_monitor: | False |
| very\_high\_throughput: | True |
| zone: | Outdoor |

RF Group: Celje WiFi

|  |  |
| --- | --- |
|  |  |
| allowed\_channels: | 100,104,120,124 |
| beacon\_interval: | 100 |
| ch\_bw\_range: | ['20MHz', '40MHz'] |
| channel\_quality\_aware: | False |
| channel\_quality\_threshold: | 70 |
| channel\_quality\_wait\_time: | 120 |
| csa\_count: | 0 |
| disable\_arm\_wids\_functions: | off |
| dot11h: | False |
| dpp\_configurator\_connectivity: | False |
| frame\_bursting\_mode: | dynamic |
| high\_noise\_backoff\_time: | 720 |
| interference\_immunity: | 2 |
| legacy\_mode: | False |
| max\_tx\_power: | 51 |
| max\_tx\_power\_ai: | false |
| min\_tx\_power: | 51 |
| min\_tx\_power\_ai: | false |
| name: | Mesh |
| radar\_backoff\_time: | 720 |
| rts\_mode: | default |
| scanning\_disable: | True |
| smart\_antenna: | False |
| spectrum\_band: |  |
| spectrum\_monitor: | False |
| very\_high\_throughput: | True |
| zone: | Mesh |

RF Group: Celje WiFi

|  |  |
| --- | --- |
|  |  |
| allowed\_channels: | 36,40,44,48,52,56,60,64,100,104,108,112,116,120,124,128,132,136,140,149,153,157,161,165 |
| beacon\_interval: | 100 |
| ch\_bw\_range: | ['20MHz', '80MHz'] |
| channel\_quality\_aware: | False |
| channel\_quality\_threshold: | 70 |
| channel\_quality\_wait\_time: | 120 |
| csa\_count: | 0 |
| disable\_arm\_wids\_functions: | dynamic |
| dot11h: | False |
| dpp\_configurator\_connectivity: | False |
| frame\_bursting\_mode: | dynamic |
| high\_noise\_backoff\_time: | 720 |
| interference\_immunity: | 2 |
| legacy\_mode: | False |
| max\_tx\_power: | 21 |
| max\_tx\_power\_ai: | false |
| min\_tx\_power: | 15 |
| min\_tx\_power\_ai: | false |
| name: | default |
| radar\_backoff\_time: | 720 |
| rts\_mode: | default |
| scanning\_disable: | True |
| smart\_antenna: | False |
| spectrum\_band: |  |
| spectrum\_monitor: | False |
| very\_high\_throughput: | True |
| zone: |  |