Configuration group  
Stari grad Celje

Mestna občina Celje  
  
Konfiguracija 2024-02-23

WLAN: Barbara

|  |  |
| --- | --- |
|  |  |
| user\_bridging: | False |
| deny\_intra\_vlan\_traffic: | False |
| very\_high\_throughput\_disable: | True |
| high\_throughput\_disable: | True |
| high\_efficiency\_disable: | True |
| tspec: | False |
| tspec\_bandwidth: | 2000 |
| strict\_svp: | False |
| use\_ip\_for\_calling\_station: | False |
| called\_station\_id\_type: | macaddr |
| wmm\_background\_dscp: |  |
| wmm\_best\_effort\_dscp: |  |
| wmm\_video\_dscp: |  |
| wmm\_voice\_dscp: |  |
| auth\_req\_threshold: | 0 |
| dot11r: | False |
| mdid: | 1 |
| dot11k: | True |
| dot11v: | False |
| mac\_authentication\_delimiter: |  |
| mac\_authentication\_upper\_case: | False |
| auth\_pkt\_delimiter: |  |
| zone: |  |
| explicit\_ageout\_client: | False |
| opmode\_transition\_disable: | True |
| download\_role: | False |
| wmm\_uapsd: | True |
| management\_frame\_protection: | False |
| gw\_profile\_name: |  |
| cluster\_name: |  |
| dmo\_client\_threshold: | 6 |
| ftm\_responder\_enable: | True |
| cluster\_group\_name: |  |
| secondary\_cluster\_name: |  |
| secondary\_cluster\_group\_name: |  |
| cluster\_preemption: | False |
| mpsk\_local\_profile: |  |
| rrm\_quiet\_ie: | True |
| disable\_6ghz\_on\_mesh: | False |
| rf\_band\_6ghz: | False |
| a\_beacon\_rate: | default |
| g\_beacon\_rate: | default |
| advertise\_ap\_name: | False |
| reconnect\_client\_on\_failover: | False |
| forward\_mode: | bridge |
| default\_role: |  |
| pmk\_cache: | True |
| captive\_portal: | disable |
| captive\_profile\_name: |  |
| captive\_exclude: | [] |
| captive\_portal\_proxy\_ip: |  |
| captive\_portal\_proxy\_port: |  |
| called\_station\_id\_incl\_ssid: | False |
| called\_station\_id\_deli: |  |
| auth\_pkt\_upper\_case: | False |
| name: | Barbara |
| essid: | Barbara |
| type: | employee |
| content\_filtering: | False |
| enforce\_dhcp: | False |
| wispr: | False |
| hide\_ssid: | False |
| mac\_authentication: | False |
| rf\_band: | all |
| inactivity\_timeout: | 1000 |
| multicast\_rate\_optimization: | False |
| broadcast\_filter: | arp |
| dtim\_period: | 1 |
| dynamic\_multicast\_optimization: | False |
| work\_without\_uplink: | False |
| dmo\_channel\_util\_threshold: | 90 |
| air\_time\_limit: |  |
| bandwidth\_limit: |  |
| per\_user\_limit: |  |
| wmm\_background\_share: | 0 |
| wmm\_best\_effort\_share: | 0 |
| wmm\_video\_share: | 0 |
| wmm\_voice\_share: | 0 |
| g\_min\_tx\_rate: | 12 |
| g\_max\_tx\_rate: | 54 |
| a\_min\_tx\_rate: | 18 |
| a\_max\_tx\_rate: | 54 |
| max\_clients\_threshold: | 64 |
| local\_probe\_req\_threshold: | 0 |
| vlan: | SGC-Zaposleni |
| opmode: | wpa2-psk-aes |
| termination: | False |
| reauth\_interval: | 0 |
| blacklist: | False |
| leap\_use\_session\_key: | False |
| l2\_auth\_failthrough: | False |
| max\_auth\_failures: | 0 |
| radius\_accounting: | False |
| radius\_interim\_accounting\_interval: | 0 |
| radius\_accounting\_mode: | user-authentication |
| server\_load\_balancing: | False |
| l2switch\_mode: | False |
| hotspot\_profile: |  |
| local\_probe\_req\_threshold\_ai: | false |
| auth\_req\_threshold\_ai: | false |
| air\_time\_limit\_cb: | False |
| bandwidth\_limit\_cb: | False |
| per\_user\_limit\_cb: | False |
| disable\_ssid: | False |
| okc: | False |
| time\_range\_profiles\_status: | [] |
| auth\_server1: | InternalServer |
| auth\_server2: |  |
| accounting\_server1: |  |
| accounting\_server2: |  |
| auth\_survivability: | False |
| priority\_use\_local\_cache\_auth: | False |
| cloud\_guest: | False |
| cloud\_auth: | False |
| auth\_cache\_timeout: | 24 |
| wpa\_passphrase: | \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* |
| wep\_key: |  |
| wep\_index: | 0 |
| set\_role\_machine\_auth\_machine\_only: |  |
| set\_role\_machine\_auth\_user\_only: |  |
| set\_role\_pre\_auth: |  |
| set\_role\_mac\_auth: |  |
| roles: | [] |
| dynamic\_vlans: | [] |
| oos\_def: | vpn-down |
| oos\_name: | none |
| oos\_time: | 30 |
| ssid\_encoding: | utf8 |
| index: | 1 |
| access\_type: | unrestricted |
| dpp: | False |

WLAN: Celje WiFi

|  |  |
| --- | --- |
|  |  |
| user\_bridging: | False |
| deny\_intra\_vlan\_traffic: | False |
| very\_high\_throughput\_disable: | True |
| high\_throughput\_disable: | True |
| high\_efficiency\_disable: | True |
| tspec: | False |
| tspec\_bandwidth: | 2000 |
| strict\_svp: | False |
| use\_ip\_for\_calling\_station: | False |
| called\_station\_id\_type: | macaddr |
| wmm\_background\_dscp: |  |
| wmm\_best\_effort\_dscp: |  |
| wmm\_video\_dscp: |  |
| wmm\_voice\_dscp: |  |
| auth\_req\_threshold: | 0 |
| dot11r: | False |
| mdid: | 1 |
| dot11k: | True |
| dot11v: | False |
| mac\_authentication\_delimiter: | : |
| mac\_authentication\_upper\_case: | True |
| auth\_pkt\_delimiter: |  |
| zone: |  |
| explicit\_ageout\_client: | False |
| opmode\_transition\_disable: | True |
| download\_role: | False |
| wmm\_uapsd: | True |
| management\_frame\_protection: | False |
| gw\_profile\_name: |  |
| cluster\_name: |  |
| dmo\_client\_threshold: | 6 |
| ftm\_responder\_enable: | True |
| cluster\_group\_name: |  |
| secondary\_cluster\_name: |  |
| secondary\_cluster\_group\_name: |  |
| cluster\_preemption: | False |
| mpsk\_local\_profile: |  |
| rrm\_quiet\_ie: | True |
| disable\_6ghz\_on\_mesh: | False |
| rf\_band\_6ghz: | False |
| a\_beacon\_rate: | default |
| g\_beacon\_rate: | default |
| advertise\_ap\_name: | False |
| reconnect\_client\_on\_failover: | False |
| forward\_mode: | bridge |
| default\_role: |  |
| pmk\_cache: | True |
| captive\_portal: | external |
| captive\_profile\_name: | Celje Centralka\_#guest#\_ |
| captive\_exclude: | [] |
| captive\_portal\_proxy\_ip: |  |
| captive\_portal\_proxy\_port: |  |
| called\_station\_id\_incl\_ssid: | False |
| called\_station\_id\_deli: |  |
| auth\_pkt\_upper\_case: | False |
| name: | Celje WiFi |
| essid: | Celje WiFi |
| type: | guest |
| content\_filtering: | False |
| enforce\_dhcp: | True |
| wispr: | False |
| hide\_ssid: | False |
| mac\_authentication: | True |
| rf\_band: | all |
| inactivity\_timeout: | 1000 |
| multicast\_rate\_optimization: | True |
| broadcast\_filter: | arp |
| dtim\_period: | 1 |
| dynamic\_multicast\_optimization: | True |
| work\_without\_uplink: | False |
| dmo\_channel\_util\_threshold: | 90 |
| air\_time\_limit: |  |
| bandwidth\_limit: |  |
| per\_user\_limit: |  |
| wmm\_background\_share: | 0 |
| wmm\_best\_effort\_share: | 0 |
| wmm\_video\_share: | 0 |
| wmm\_voice\_share: | 0 |
| g\_min\_tx\_rate: | 18 |
| g\_max\_tx\_rate: | 54 |
| a\_min\_tx\_rate: | 24 |
| a\_max\_tx\_rate: | 54 |
| max\_clients\_threshold: | 64 |
| local\_probe\_req\_threshold: | 0 |
| vlan: | SGC-Gosti |
| opmode: | opensystem |
| termination: | False |
| reauth\_interval: | 0 |
| blacklist: | False |
| leap\_use\_session\_key: | False |
| l2\_auth\_failthrough: | False |
| max\_auth\_failures: | 0 |
| radius\_accounting: | True |
| radius\_interim\_accounting\_interval: | 5 |
| radius\_accounting\_mode: | user-authentication |
| server\_load\_balancing: | False |
| l2switch\_mode: | False |
| hotspot\_profile: |  |
| local\_probe\_req\_threshold\_ai: | false |
| auth\_req\_threshold\_ai: | false |
| air\_time\_limit\_cb: | False |
| bandwidth\_limit\_cb: | False |
| per\_user\_limit\_cb: | False |
| disable\_ssid: | False |
| okc: | False |
| time\_range\_profiles\_status: | [] |
| auth\_server1: | AS1\_#guest#\_ |
| auth\_server2: | AS2\_#guest#\_ |
| accounting\_server1: |  |
| accounting\_server2: |  |
| auth\_survivability: | False |
| priority\_use\_local\_cache\_auth: | False |
| cloud\_guest: | True |
| cloud\_auth: | False |
| auth\_cache\_timeout: | 24 |
| wpa\_passphrase: |  |
| wep\_key: |  |
| wep\_index: | 0 |
| set\_role\_machine\_auth\_machine\_only: |  |
| set\_role\_machine\_auth\_user\_only: |  |
| set\_role\_pre\_auth: | Celje Centralka\_#guest#\_ |
| set\_role\_mac\_auth: |  |
| roles: | [] |
| dynamic\_vlans: | [] |
| oos\_def: | vpn-down |
| oos\_name: | none |
| oos\_time: | 30 |
| ssid\_encoding: | utf8 |
| index: | 2 |
| access\_type: | unrestricted |
| dpp: | False |